[module/battery]
type = internal/battery
battery = BAT1
adapter = ACAD
full-at = 100

format-charging = <label-charging>

format-discharging = <ramp-capacity>  <label-discharging>

label-charging =   %percentage%%

label-discharging = %percentage%%

ramp-capacity-0 = 
ramp-capacity-1 = 
ramp-capacity-2 = 
ramp-capacity-3 = 
ramp-capacity-4 = 
ramp-capacity-5 = 
ramp-capacity-6 = 
ramp-capacity-7 = 
ramp-capacity-8 = 
ramp-capacity-9 = 
ramp-capacity-10 = 

[module/title]
type = internal/xwindow
label-maxlen = 50
[module/temperature]
type = internal/temperature

; for i in /sys/class/thermal/thermal_zone*; do echo "$i: $(<$i/type)"; done
thermal-zone = /sys/class/thermal/thermal_zone0

hwmon-path = /sys/devices/pci0000:00/0000:00:01.1/0000:10:00.0/hwmon/hwmon2/temp1_input

; for i in /sys/class/hwmon/hwmon*/temp*_input; do echo "$(<$(dirname $i)/name): $(cat ${i%_*}_label 2>/dev/null || echo $(basename ${i%_*})) $(readlink -f $i)"; done
format = <label>

label = %temperature-c%

[module/wlan]
type = internal/network
interface = wlp1s0
interval = 3.0

format-connected = <label-connected>

label-connected =  %essid%

format-disconnected = <label-disconnected>

label-disconnected = 

[module/wireguard]
type = custom/script

exec = ~/.config/polybar/wireguard-is-connected.sh

click-left = ~/.config/polybar/toggle-wireguard.sh

interval = 5

[module/eth]
type = internal/network
interface = enp34s0

interval = 3.0

label-connected =  %downspeed%

format-connected = <label-connected>

label-disconnected =  

[module/phone-battery]
type = custom/script

exec = echo " $(mconnectctl show-battery /org/mconnect/device/1 | head -1 | awk '{print $2}')%"

exec-if = ~/.config/polybar/phone-is-connected.sh

interval = 300

[module/date]
type = internal/date
interval = 5

time = %H:%M

date = %a %e %b

label = %date% %time%

format =  <label>
